# Sommerhuber, Foot basin square

## Item no. 651 261

Foot basin square made of heat storage ceramic in one single piece without joints,
glazed inside and outside over the entire surface,
coning form with a drain located in the middle

\* top size W/L/H: ~49/49/30cm

\* waved ground
\* glazing in accordance to the current glaze overview

\* spillway hole in the ceramic and mounting kit excluded

\* to mount on the floor directly
\* drain trap needs to be built on site

\* optional discharge; two possibilities:

* with standpipe valve
* with hole drilling in the ceramic

Installation, maintenance and cleaning in accordance to the product data sheet
of manufacturer