# Sommerhuber, Foot basin round

## Item no. 651 263

Foot basin round made of heat storage ceramic in one single piece without joints,  
glazed inside and outside over the entire surface,  
coning form with a drain located in the middle

\* top size W/H: ~⌀ 49/30cm

\* waved ground

\* glazing in accordance to the current glaze overview

\* spillway hole in the ceramic and mounting kit excluded

\* to mount on the floor directly  
\* drain trap needs to be built on site

\* optional discharge; two possibilities:

* with standpipe valve
* with hole drilling in the ceramic

Installation, maintenance and cleaning in accordance to the product data sheet  
of manufacturer