# Sommerhuber wet-room seats

# Wet-room seats made of heat storage ceramics with one transverse joint only.Consisting of backrest, seat and plinth.including EPS sub-construction

# For optimal heat sensation and relaxation the backrest ceramic.is designed up to slightly over head level.

\* height ~141 cm

\* depth ~61 cm

# \* in three width dimensions (nominal size ~ 45/61/72 cm )  as well as two corner parts of 22,5° and 45°

# \* seat with 1° inclination to avoid wet spots

# \* glazing in accordance to the current glaze overview\* individual cutting to length in accordance to exact measurements

# Installation needs to be done by skilled staff in accordance to assembly recommendation of manufacturer.\* optional electrical or water heating\* optional LED illumination