**Sommerhuber, Lounger One**

Item no. 650 000

Heated lounger finished with heat storage ceramic and 2 transverse joints only,
incl. EPS sub-construction

\* size ~ 100x66x185 cm

\* weight ~ 87 kg

\* static load up to 250kg, if completely glued to the ground

\* electrically heated with a EU 230V heating system,

 heat capacity 709W

\* one zone electrical heating

\* power supply via floor

\* incl. thermostat for external installation

\* incl. cable (standard length 2,5m)

\* incl. bolster

\* glazing in accordance to the current glaze overview

Ready to plug in product

\* optional LED illumination