# Sommerhuber dry-room seats

# Dry-room seats made of heat storage ceramics with one transverse joint only. Consisting of backrest, seat and plinth. For optimal heat sensation and relaxation the backrest ceramic is designed up to slightly over head level. including EPS sub-construction

\* height ~135 cm

\* depth ~88 cm

# \* in three width dimensions (nominal size ~ 45/61/72 cm ) as well as two corner parts of 22,5° and 45°

# \* deep shaped seat for relaxed sitting position \* glazing in accordance to the current glaze overview \* individual cutting to length in accordance to exact measurements

# Installation needs to be done by skilled staff in accordance to assembly recommendation of manufacturer.

# \* optional electrical or water heating \* optional LED illumination