# Sommerhuber, Floating Bench edged

Item No, 694 40., 694 8..

**Floating Benches made of heat storage ceramics in edged style**

incl. V4A stainless steel cantilever console for subconstruction

**\* height ~11 cm**

**\* depth: in 3 dimensions (nominal size ~ 45/53/75 cm)**

**\* width: in 5 dimensions (nominal size ~** 45/75/90/143/150 cm**)**

**\* Material compound of cantilever console + 4 mm V4A sheet steel + adhesive with heating + 18 mm   
 ceramic ensures: Static load up to 175 kg with distance between consoles max. 75 cm**

**\* glazing in accordance to the current glaze overview  
\* individual cutting to length in accordance to exact measurements**

**Installation needs to be done by skilled staff in accordance to assembly   
recommendation of manufacturer.**

# \* optional LED light

**Assembly - Sommerhuber, Floating Bench edged**

**Installation Floating Bench edged in accordance to assembly recommendation.**