**Sommerhuber, Lounger Two**

**Headsection inserted into wall and foot-section freestanding**

**Item no. 651 001**

**Version: head- and foot-section freestanding (item no. 8225506)**

**Levitated heated lounger finished with heat storage ceramic and 2 transverse joints only,  
incl. stainless steel V2A sub-construction covered with EPS corpus**

\* size ~85x69x200cm

\* weight ~145kg

\* static weight capacity up to 250kg

\* electrically heated with a EU 230V heating system,

heat capacity 739W, heating system mounted

\* one zone electrical heating

\* power supply via floor

\* incl. thermostat for external installation

\* incl. cable (standard length 2,5m)

\* incl. bolster “Relax”

\* glazing in accordance to the current glaze overview

**Delivery in separate components, pre-assembled,  
installation in accordance to assembly recommendation**

\* optional LED illumination

**Assembly - Sommerhuber, Lounger Two**

**Installation levitated heated Lounger Two, head- and foot-section freestanding,  
in accordance to assembly recommendation.**