# Sommerhuber, Additional part to rectangular size

## Item no. 651 265

Additional part to the foot basin square (item no. 651 261) to fix fittings

made of heat storage ceramic in one single piece without joints,  
glazed inside and outside over the entire surface, coning form

\* top size W/L/H: ~15/49/30cm

\* glazing in accordance to the current glaze overview

\* holes drilled sharp-edged, in accordance to exact measurements